Uvod u računalne mreže - Lab 9: “IPv4 Subnetiranje-uvod”

Za zadatak koristite Wordpad alat i surađujte s kolegama i nastavnikom, kada odgovorite na sva pitanja uplodajte vježbu pod Seminarski rad. 

ZADATAK

1. Pretvorite subnet masku u binarni oblik, a zatim je zapišite u obliku prefiksa (/x)
a)	255.255.255.0 – 11111111.11111111.11111111.00000000 - /24
b)	255.255.252.0 – 11111111.11111111.11111100.00000000 - /22
c)	255.252.0.0 – 11111111.11111100.00000000.00000000 - /14
d)	255.255.255.224 – 11111111.11111111.11111111. 11100000 - /27
e)	255.255.255.128 – 11111111.11111111.11111111.10000000 - /25
f)	255.255.255.192 – 11111111.11111111.11111111.11000000 - /26
g)	255.255.255.240 – 11111111.11111111.11111111. 11110000 - /28
h)	255.240.0.0 – 11111111.11110000.00000000.00000000
i)	255.0.0.0 – 11111111.00000000.00000000.00000000 - /8
j)	128.0.0.0 – 10000000.00000000.00000000.00000000 - /1
k)	255.192.0.0 – 11111111.11000000.00000000.00000000 - /10

2. Pretvorite subnet masku u binarni i decimalni oblik i dodatno zapišite za koliko korisnika je pojedina subnet maska
a)	/29 – 11111111.11111111.11111111.11111000 – 255.255.255.248 – 6 hostova
b)	/28 – 11111111.11111111.11111111.11110000 – 255.255.255.240 – 14 hostova
c)	/15 – 11111111.11111110.00000000.00000000 – 255.254.0.0 - 131,068 hostova
d)	/13 – 11111111.11111000.00000000.00000000 – 255.248.0.0 - 524,272 hostova
e)	/26 – 11111111.11111111.11111111.11000000 – 255.255.255.192 – 62 hostova
f)	/24 – 11111111.11111111.1111111.0 - 255.255.255.0 – 254 hostova
g)	/19 – 11111111.11111111.11100000.00000000 – 255.255.224.0 - 8,128 hostova
h)	/12 – 11111111.11110000.00000000.00000000 – 255.240.0.0 - 1,048,544 hostova
i)	/23 – 11111111.11111111.1111110.00000000 – 255.255.254.0 – 508 hostova
j)	/22 – 11111111.11111111.11111100.00000000 – 255.255.252.0 - 1,016 hostova
k)	/29 – 11111111.11111111.11111111.11111000 – 255.255.255.248 – 6 hostova
l)	/14 – 11111111.11111100.00000000.00000000 – 255.252.0.0 - 262,136 hostova
m)	/18 – 11111111.11111111.11000000.00000000 – 255.255.192.0 - 16,256 hostova

3. Pretvorite IP adresu u binarni oblik
a)	192.168.25.13 – 11000000.10101000.00011001.00001101
b)	192.168.44.55 - 11000000.10101000.00101100.00110111
c)	192.168.100.207 - 11000000.10101000.01100100.11001111
d)	10.20.30.161 - 00001010.00010100.00011110.10100001
e)	10.50.70.159 - 00001010.00110010.01000110.10011111
f)	10.100.200.198 - 00001010.01100100.11001000.11000110
g)	172.16.10.192 - 10101100.00010000.00001010.11000000
h)	172.16.20.225 - 10101100.00010000.00010100.11100001
i)	172.16.30.66 - 10101100.00010000.00011110.01000010

Za pripremu i dodatno učenje

Potražiti na Udemy  Section 3 (Bonus video 1 prvi i drugi dio i bonus video 2) (10+6+6 minuta)-proći sve prije ispita)

IP address network and host portion | subnet mask explained | ccna 200-301 free | (4 min)
https://youtu.be/eHV1aOnu7oM

IPv4 Addressing Lesson 1: Binary and the IP Address MADE EASY (15 min)
https://youtu.be/ddM9AcreVqY

IPv4 Addressing Lesson 2: Network IDs and Subnet Masks. (21 min)
https://youtu.be/XQ3T14SIlV4

IPv4 Addressing Lesson 3: The Class System (11 min)
https://youtu.be/4xlzlgYGqW8